HOWTO run with the new DAS and sparc based IDS ICS

This note sets out the steps needed to run up the new Sparc ICS control system.

1. Log on to the INT observing system Sparc20 (lpss12) with username observer (password as given on the monitor).

2. In the xterm window type obssys (this only needs to be done once, it sets up environment variables and so forth).

3. Select the relevant option for the currently configured system (from the list)

4. Start the observing system (DAS + ICS) with the command startobssys. Many windows pop up including:

Talker system messages CCD status Info for the CCD (part of the DAS) Observing Log log file — info here ends up in your hardcopy log INT Cass Mimic Graphical display of the IDS xterm and the xterm where you can type DAS and IDS + A&G commands

5. You can then setup ccd tek3 to prepare the CCD and carry on as outlined in the DAS, IDS and A&G user manuals (to be found in the INT ’most excellent book’ black folder).

6. In case of problems the best course of action is to shutdown the systems with the command shutdownobssys from the xterm window. Then start up the observing system again as outlined above. The shutdown command can also be used at the end of observing.

7. All run and instrument commands can be entered in the xterm window. Commands can be strung together with the ; character (e.g. compmirror in ; complamps CuNe)

Nicholas A Walton Version 1.1 (19 June 1997) (INT Telescope Manager)