Appendix B

wyffos filters

B.1 Available Filters

Due to the unusual physical dimensions of the wyffos slit, filters used in the spectrograph are expensive and difficult to obtain. Currently (02/1999), four broad-band order sorting filters are available for use in reflection mode (top graph of accompanying figure), and a further five are available for order isolation in echelle mode. The echelle filters have interference coatings and have been selected to isolate important astrophysical diagnostics (e.g. Hα).

Focus offsets

The corrections to the slitfocus for the filter thicknesses are:-

Table B.1: filter table Filter identification Thickness Focus Offset (mm) (μm)

BG39 3.00 +1000 GG495 3.00 +1000 OG530 3.00 +1000 RG630 3.00 +1000

Echelle Filters 8830Å(order 3) 6.00 +2000 6625Å(order 4) 6.10 +2003 5300Å(order 5) 4.12 +1373 4415Å(order 6) 6.10 +2003 3785Å(order 7) 5.90 +1997

55

56 APPENDIX B. WYFFOS FILTERS

Figure B.1: filter scans