R316R Grating

Table 1: Copper-Argon Lamp with R316R

Range (Å) Exp. (s) Filter Disp (Å/pixel) Lines RMS (Å) 5987-7513 3 GG495 1.4716 21 0.0692 7502-9028 1 GG495 1.4805 17 0.0704 8797-10323 2 RG630 1.4795 8 0.1003

Table 2: Copper-Neon Lamp with R316R

Range (Å) Exp. (s) Filter Disp (Å/pixel) Lines RMS (Å) 5987-7513 1 GG495 1.4717 27 0.0417 7502-9028 10 GG495 1.4797 23 0.0526 8797-10323 20 RG630 1.4824 14 0.0634

Table 3: Copper-Argon and Copper-Neon Lamps with R316R

Range (Å) Exp. (s) Filter Disp (Å/pixel) Lines RMS (Å) 5987-7513 1 GG495 1.4717 41 0.0799 7502-9028 1 GG495 1.4797 27 0.1041 8797-10323 2 RG630 1.4824 17 0.1130

Figure 1: Copper-Argon Lamp with R316R. Central wavelength = 6750 Å.

Figure 2: Copper-Argon Lamp with R316R. Central wavelength = 8265 Å.

Figure 3: Copper-Argon Lamp with R316R. Central wavelength = 9560 Å.

Figure 4: Copper-Neon Lamp with R316R. Central wavelength = 6750 Å.

Figure 5: Copper-Neon Lamp with R316R. Central wavelength = 8265 Å.

Figure 6: Copper-Neon Lamp with R316R. Central wavelength = 9560 Å.

Figure 7: Copper-Neon & Copper-Argon Lamps with R316R. Central wavelength = 6750 Å.

Figure 8: Copper-Neon & Copper-Argon Lamp with R316R. Central wavelength = 8265 Å.

Figure 9: Copper-Neon & Copper-Argon Lamp with R316R. Central wavelength = 9560 Å.