R600R Grating

Table 1: Copper-Argon Lamp with R600R

Range (Å) Exp. (s) Filter Disp (Å/pixel) Lines RMS (Å) 5998-6765 80 GG495 0.788 32 0.055 6790-7559 4 GG495 0.791 24 0.046 7574-8346 4 GG495 0.793 10 0.045 8366-9140 4 GG495 0.795 11 0.065

Table 2: Copper-Neon Lamp with R600R

Range (Å) Exp. (s) Filter Disp (Å/pixel) Lines RMS (Å) 5998-6765 8 GG495 0.788 19 0.033 6790-7559 8 GG495 0.791 13 0.090 7573-8346 60 GG495 0.794 15 0.069 8367-9140 20 GG495 0.795 20 0.039

Table 3: Copper-Argon and Copper-Neon Lamps with R600R

Range (Å) Exp. (s) Filter Disp (Å/pixel) Lines RMS (Å) 5998-6765 8 GG495 0.789 31 0.065 6790-7559 4 GG495 0.791 36 0.067 7574-8346 2 GG495 0.793 17 0.074 8367-9140 4 GG495 0.795 22 0.057

Figure 1: Copper-Argon Lamp with R600R. Central wavelength = 6400 Å.

Figure 2: Copper-Argon Lamp with R600R. Central wavelength = 7190 Å.

Figure 3: Copper-Argon Lamp with R600R. Central wavelength = 7980 Å.

Figure 4: Copper-Argon Lamp with R600R. Central wavelength = 8770 Å.

Figure 5: Copper-Neon Lamp with R600R. Central wavelength = 6400 Å.

Figure 6: Copper-Neon Lamp with R600R. Central wavelength = 7190 Å.

Figure 7: Copper-Neon Lamp with R600R. Central wavelength = 7980 Å.

Figure 8: Copper-Neon Lamp with R600R. Central wavelength = 8770 Å.

Figure 9: Copper-Neon & Copper-Argon Lamps with R600R. Central wavelength = 6400 Å.

Figure 10: Copper-Neon & Copper-Argon Lamp with R600R. Central wavelength = 7190 Å.

Figure 11: Copper-Neon & Copper-Argon Lamp with R600R. Central wavelength = 7980 Å.

Figure 12: Copper-Neon & Copper-Argon Lamp with R600R. Central wavelength = 8770 Å.